IfcCableCarrierFittingTypeEnum

Definition from IAI: The IfcCableCarrierFittingTypeEnum defines the range of different types of cable carrier fitting that can be specified.

> HISTORY: New type in IFC 2x2

Enumeration

Value | Definition | Pset
BEND | A fitting that changes the route of the cable carrier. | NO
CROSS | A fitting at which two branches are taken from the main route of the cable carrier simultaneously. | NO
REDUCER | A fitting that changes the physical size of the main route of the cable carrier. | NO
TEE | A fitting at which a branch is taken from the main route of the cable carrier. | NO
USERDEFINED |  |
NOTDEFINED |  |

EXPRESS specification:

TYPE IfcCableCarrierFittingTypeEnum = ENUMERATION OF
( | BEND, CROSS, REDUCER, TEE, USERDEFINED, NOTDEFINED);
END_TYPE;