IfcFlowInstrumentTypeEnum

Definition from IAI: The IfcFlowInstrumentTypeEnum defines the range of different types of flow instrument that can be specified.

> HISTORY: New type in IFC 2x2

Enumeration

Value | Definition | Pset
PRESSUREGAUGE | A device that reads and displays a pressure value at a point or the pressure difference between two points. | YES
THERMOMETER | A device that reads and displays a temperature value at a point. | YES
AMMETER | A device that reads and displays the current flow in a circuit. | NO
FREQUENCYMETER | A device that reads and displays the electrical frequency of an alternating current circuit. | NO
PHASEANGLEMETER | A device that reads and displays the phase angle of a phase in a polyphase electrical circuit. | NO
POWERFACTORMETER | A device that reads and displays the power factor of an electrical circuit. | NO
VOLTMETER_PEAK | A device that reads and displays the peak voltage in an electrical circuit. | NO
VOLTMETER_RMS | A device that reads and displays the RMS (mean) voltage in an electrical circuit. | NO
USERDEFINED |  |
NOTDEFINED |  |

EXPRESS specification:

TYPE IfcFlowInstrumentTypeEnum = ENUMERATION OF
( | PRESSUREGAUGE, THERMOMETER, AMMETER, FREQUENCYMETER, POWERFACTORMETER, PHASEANGLEMETER, VOLTMETER_PEAK, VOLTMETER_RMS, USERDEFINED, NOTDEFINED);
END_TYPE;