IfcThermalLoadTypeEnum

Definition from IAI: This enumeration defines the type of thermal load for spaces or zones, as derived from various use cases:

- SENSIBLE: Energy added or removed from air that affects its temperature.
- LATENT: Energy added or removed from air that affects its humidity or concentration of water vapor.
- RADIANT: Electromagnetic energy added or removed by emission or absorption.
- NOTDEFINED: Undefined thermal load type.

> HISTORY: New enumeration in IFC R2x2.

EXPRESS specification:

TYPE IfcThermalLoadTypeEnum = ENUMERATION OF
( | SENSIBLE, LATENT, RADIANT, NOTDEFINED);
END_TYPE;