IfcSanitaryTerminalTypeEnum

Definition from IAI: The IfcSanitaryTerminalTypeEnum defines the range of different types of sanitary terminal that can be specified.

> HISTORY: New type in IFC 2x2

Enumeration

Value | Definition | Pset
BATH | Sanitary appliance for immersion of the human body or parts of it (BS6100). | YES
BIDET | Waste water appliance for washing the excretory organs while sitting astride the bowl (BS6100) | YES
CISTERN | A water storage unit attached to a sanitary terminal that is fitted with a device, operated automatically or by the user, that discharges water to cleanse a water closet (toilet) pan, urinal or slop hopper. (BS6100) | YES
SHOWER | Installation or waste water appliance that emits a spray of water to wash the human body (BS6100). | YES
SINK | Waste water appliance for receiving, retaining or disposing of domestic, culinary, laboratory or industrial process liquids. | YES
SANITARYFOUNTAIN | A sanitary terminal that provides a low pressure jet of water for a specific purpose (IAI). | YES
TOILETPAN | Soil appliance for the disposal of excrement. | YES
URINAL | Soil appliance that receives urine and directs it to a waste outlet (BS6100) | YES
WASHHANDBASIN | Waste water appliance for washing the upper parts of the body. (BS6100) | YES
WCSEAT | Hinged seat that fits on the top of a water closet (WC) pan. (BS6100) | YES
USERDEFINED |  |
NOTDEFINED |  |

EXPRESS specification:

TYPE IfcSanitaryTerminalTypeEnum = ENUMERATION OF
( | BATH, BIDET, CISTERN, SHOWER, SINK, SANITARYFOUNTAIN, TOILETPAN, URINAL, WASHHANDBASIN, WCSEAT, USERDEFINED, NOTDEFINED);
END_TYPE;