#### 5.2.4.26 AISC_EM11_Pset_TubeOffshoreSaddle

| Tube Offshore Saddle: An offshore saddle can be compared with a normal saddle, except that in the heel zone the fit line of the profile has been transformed to the outside of the cut pipe. It is called offshore saddle as this saddle is widely used in the offshore. Most of these profiles comply with the standards set in the American Welding Standard (AWS). image source : Tube NC

buildingSMART Data Dictionary

PSD-XML

Name | Type | Description
--- | --- | ---
Type | P_SINGLEVALUE / IfcIdentifier |
MinBurnAngle | P_SINGLEVALUE / IfcPlaneAngleMeasure |
MaxBurnAngle | P_SINGLEVALUE / IfcPlaneAngleMeasure |
Bevel | P_SINGLEVALUE / IfcPlaneAngleMeasure | The bevel is nothing more than a kerf with a continuous opening angle between the cut and connecting material. Internally in the machine software the bevel is created mathematically by calculating the dihedral angle and subtracting the bevel from it.
RootOpening | P_SINGLEVALUE / IfcPositiveLengthMeasure |
Shrinkage | P_SINGLEVALUE / IfcPositiveLengthMeasure |
Side | P_ENUMERATEDVALUE / AISC_EM11_CriticalFace |

Link to this page