#### 5.2.4.10 AISC_EM11_Pset_SurfaceTreatment

| Surface Treatment: Surface Treatment represents blasted, galvanized, painted, primed and etc on Assembly or Element. Covering may have optional geometric representation if the covering only applied partially. In this regards, Assembly cannot have partial covering as it does not have geometric representation by definition. Therefore, partial covering should be applied to its components. This rule applied to all other element without geometric representation. An element may have multiple coverings, which should have sequential order number that shows application order.

buildingSMART Data Dictionary

PSD-XML

Name | Type | Description
--- | --- | ---
SurfaceTreatement | P_LISTVALUE / IfcIdentifier |
| Surface Treatment | An element may have multiple coverings, which should have sequential order number that shows application order. Possible values include and not limited to: Blast Painted Galvanized Primed

Link to this page