IfcSwitchingDeviceTypeEnum

Definition from IAI: The IfcSwitchingDeviceTypeEnum defines the range of different types of switch that can be specified.

> HISTORY: New type in IFC 2x2

Enumeration

Value | Definition | Pset
CONTACTOR | An electrical device used to control the flow of power in a circuit on or off. | YES
EMERGENCYSTOP | An emergency stop device acts to remove as quickly as possible any danger that may have arisen unexpectedly. | YES
STARTER | A starter is a switch which in the closed position controls the application of power to an electrical device. | YES
SWITCHDISCONNECTOR | A switch disconnector is a switch which in the open position satisfies the isolating requirements specified for a disconnector. | YES
TOGGLESWITCH | A toggle switch is a switch that enables or isolates electrical power through a two position on/off action. | YES
USERDEFINED |  |
NOTDEFINED |  |

EXPRESS specification:

TYPE IfcSwitchingDeviceTypeEnum = ENUMERATION OF
( | CONTACTOR, EMERGENCYSTOP, STARTER, SWITCHDISCONNECTOR, TOGGLESWITCH, USERDEFINED, NOTDEFINED);
END_TYPE;