IfcAlarmTypeEnum

Definition from IAI: The IfcAlarmTypeEnum defines the range of different types of alarm that can be specified.

> HISTORY: New type in IFC 2x2

Enumeration

Value | Definition | Pset
BELL | An audible alarm | NO
BREAKGLASSBUTTON | An alarm activation mechanism in which a protective glass has to be broken to enable a button to be pressed. | NO
LIGHT | A visual alarm | NO
MANUALPULLBOX | An alarm activation mechanism in which activation is achieved by a pulling action. | NO
SIREN | An audible alarm | NO
WHISTLE | An audible alarm | NO
USERDEFINED |  |
NOTDEFINED |  |

EXPRESS specification:

TYPE IfcAlarmTypeEnum = ENUMERATION OF
( | BELL, BREAKGLASSBUTTON, LIGHT, MANUALPULLBOX, SIREN, WHISTLE, USERDEFINED, NOTDEFINED);
END_TYPE;