#### 5.2.4.27 AISC_EM11_Pset_TubeOffshoreChamfer

| Tube Offshore Chamfer: An offshore chamfer can be compared with a normal chamfer, except that in the heel zone the fit line of the macro has been transformed to the outside of the cut pipe. It is called offshore chamfer as this chamfer is widely used in the offshore industry. Most of these macros comply with the standards set in the American Welding Standard (AWS).

buildingSMART Data Dictionary

PSD-XML

Name | Type | Description
--- | --- | ---
Type | P_SINGLEVALUE / IfcIdentifier |
MinBurnAngle | P_SINGLEVALUE / IfcPlaneAngleMeasure |
MaxBurnAngle | P_SINGLEVALUE / IfcPlaneAngleMeasure |
Bevel | P_SINGLEVALUE / IfcPlaneAngleMeasure | The bevel is nothing more than a kerf with a continuous opening angle between the cut and connecting material. Internally in the machine software the bevel is created mathematically by calculating the dihedral angle and subtracting the bevel from it.
RootOpening | P_SINGLEVALUE / IfcLengthMeasure |
Shrinkage | P_SINGLEVALUE / IfcPositiveLengthMeasure |
Side | P_ENUMERATEDVALUE / AISC_EM11_CriticalFace |

Link to this page