IfcConditionCriterionSelect

Definition from IAI: An IfcConditionCriterionSelect enables the selection of the criterion that is to be measured or assessed to establish the condition of an artifact(s).

> HISTORY: New Select type in IFC 2x2

Select From:

- IfcLabel (for an observed or assessed criterion)
- IfcMeasureWithUnit (for a measured criterion)

EXPRESS specification:

TYPE IfcConditionCriterionSelect = SELECT
( | IfcLabel, IfcMeasureWithUnit);
END_TYPE;