IfcElectricCurrentMeasure

Definition from ISO/CD 10303-41:1992: The value for the movement of electrically charged particles.

Usually measured in Ampere (A).

Type: REAL

> NOTE Corresponding STEP name: electric_current_measure, please refer to ISO/IS 10303-41:1994 for the final definition of the formal standard.

> HISTORY New type in IFC Release 1.5.1.

EXPRESS specification:

TYPE IfcElectricCurrentMeasure = REAL;
END_TYPE;