#### 5.2.4.13 AISC_EM11_Pset_Cope

| Cope: Cope property set represents features specially at the end of part. Explicit geometry should be the base reference along with properties as additional information. This property set can be used for chamfer, flange chamfer, flange notch, or notch based on the type. image source : CIS/2 image source : CIS/2 image source : CIS/2 image source : CIS/2

buildingSMART Data Dictionary

PSD-XML

Name | Type | Description
--- | --- | ---
ChamferLength | P_SINGLEVALUE / IfcPositiveLengthMeasure |
| Chamfer Length | Chamfer length along the extrusion
ChamferDepth | P_SINGLEVALUE / IfcPositiveLengthMeasure |
| Chamfer Depth | Chamfer depth perpendicular to the extrusion
FlangeChamferLength | P_SINGLEVALUE / IfcPositiveLengthMeasure |
| Flange Chamfer Length | Flange Chamfer length along the extrusion
FlangeChamferWidth | P_SINGLEVALUE / IfcPositiveLengthMeasure |
| Flange Chamfer Width | Flange Chamfer width perpendicular to the extrusion
FlangeNotchLength | P_SINGLEVALUE / IfcPositiveLengthMeasure |
| Flange Notch Length | Flange Notch length along the extrusion
FlangeNotchWidth | P_SINGLEVALUE / IfcPositiveLengthMeasure |
| Flange Notch Width | Flange Notch width perpendicular to the extrusion
FlangeNotchRadius | P_SINGLEVALUE / IfcPositiveLengthMeasure |
| Flange Notch Radius | Flange Notch radius
NotchLength | P_SINGLEVALUE / IfcPositiveLengthMeasure |
| Notch Length | Notch length along the extrusion
NotchDepth | P_SINGLEVALUE / IfcPositiveLengthMeasure |
| Notch Depth | Notch depth perpendicular to the extrusion
NotchRadius | P_SINGLEVALUE / IfcPositiveLengthMeasure |
| Notch Radius | Notch radius

Link to this page