IfcElectricDistributionPointFunctionEnum

Definition from IAI: The IfcElectricDistributionPointTypeEnum defines the range of different functions that an electric distribution point can fulfil.

> HISTORY: New type in IFC 2x2

Enumeration

Value | Definition | Pset
ALARMPANEL | A distribution point at which alarms are annunciated. | NO
CONSUMERUNIT | A distribution point on the incoming electrical supply, typically in domestic premises, at which protective devices are located. | NO
CONTROLPANEL | A distribution point at which devices that control or monitor the operation of a site, building or part of a building are located. | NO
DISTRIBUTIONBOARD | A distribution point at which connections are made for distribution of electrical circuits usually through protective devices. | NO
GASDETECTORPANEL | A distribution point at which the detection of gas is annunciated. | NO
MIMICPANEL | A distribution point at which information that is available elsewhere is repeated or 'mimicked'. | NO
MOTORCONTROLCENTRE | A distribution point at which starting and control devices for major plant items are located. | NO
SWITCHBOARD | A distribution point at which switching devices are located. | NO
USERDEFINED |  |
NOTDEFINED |  |

EXPRESS specification:

TYPE IfcElectricDistributionPointFunctionEnum = ENUMERATION OF
( | ALARMPANEL, CONSUMERUNIT, CONTROLPANEL, DISTRIBUTIONBOARD, GASDETECTORPANEL, INDICATORPANEL, MIMICPANEL, MOTORCONTROLCENTRE, SWITCHBOARD, USERDEFINED, NOTDEFINED);
END_TYPE;