IfcCooledBeamTypeEnum

Definition from IAI: Enumeration defining the typical types of cooled beams. The IfcCooledBeamTypeEnum contains the following:

- ACTIVE: An active or ventilated cooled beam provides cooling (and heating) but can also function as an air terminal in a ventilation system.
- PASSIVE: A passive or static cooled beam provides cooling (and heating) to a room or zone.
- USERDEFINED: User-defined cooled beam type.
- NOTDEFINED: Undefined cooled beam type.

> HISTORY: New enumeration in IFC 2x2.

EXPRESS specification:

TYPE IfcCooledBeamTypeEnum = ENUMERATION OF
( | ACTIVE, PASSIVE, USERDEFINED, NOTDEFINED);
END_TYPE;