IfcOutletTypeEnum

Definition from IAI: The IfcOutletTypeEnum defines the range of different types of outlet that can be specified.

> HISTORY: New type in IFC 2x

Enumeration

Value | Definition | Pset
AUDIOVISUALOUTLET | An outlet used for an audio or visual device (include TV, radio etc.) | NO
COMMUNICATIONSOUTLET | An outlet used for connecting communications equipment (telephones, data connections) | NO
POWEROUTLET | An outlet used for connecting electrical devices requiring power. | NO
USERDEFINED |  |
NOTDEFINED |  |

EXPRESS specification:

TYPE IfcOutletTypeEnum = ENUMERATION OF
( | AUDIOVISUALOUTLET, COMMUNICATIONSOUTLET, POWEROUTLET, USERDEFINED, NOTDEFINED);
END_TYPE;