IfcSensorTypeEnum

Definition from IAI: The IfcSensorTypeEnum defines the range of different types of sensor that can be specified.

> HISTORY: New type in IFC R2.0

Enumeration

Value | Definition | Pset
CO2SENSOR | A device that senses or detects carbon dioxide. | YES
FIRESENSOR | A device that senses or detects fire. | YES
FLOWSENSOR | A device that senses or detects flow. | YES
GASSENSOR | A device that senses or detects gas. | YES
HEATSENSOR | A device that senses or detects heat. | YES
HUMIDITYSENSOR | A device that senses or detects humidity. | YES
LIGHTSENSOR | A device that senses or detects light. | YES
MOISTUREENSOR | A device that senses or detects moisture. | NO
MOVEMENTSENSOR | A device that senses or detects movement. | YES
PRESSURESENSOR | A device that senses or detects pressure. | YES
SMOKESENSOR | A device that senses or detects smoke. | YES
SOUNDSENSOR | A device that senses or detects sound. | YES
TEMPERATURESENSOR | A device that senses or detects temperature. | YES
USERDEFINED |  |
NOTDEFINED |  |

EXPRESS specification:

TYPE IfcSensorTypeEnum = ENUMERATION OF
( | CO2SENSOR, FIRESENSOR, FLOWSENSOR, GASSENSOR, HEATSENSOR, HUMIDITYSENSOR, LIGHTSENSOR, MOISTURESENSOR, MOVEMENTSENSOR, PRESSURESENSOR, SMOKESENSOR, SOUNDSENSOR, TEMPERATURESENSOR, USERDEFINED, NOTDEFINED);
END_TYPE;