IfcThermalLoadSourceEnum

Definition from IAI: This enumeration defines the various sources of thermal gains or losses for spaces or zones, derived from various use cases:

- PEOPLE: Heat gains and losses from people.
- LIGHTING: Lighting loads.
- EQUIPMENTSENSIBLE: Heat gains and losses from equipment.
- VENTILATIONINDOORAIR: Ventilation loads from indoor air.
- VENTILATIONOUTSIDEAIR: Ventilation loads from outside air.
- RECIRCULATEDAIR: Loads from recirculated air.
- EXHAUSTAIR: Loads from exhaust air.
- AIREXCHANGERATE: Loads from the air exchange rate.
- DRYBULBTEMPERATURE: Loads from the dry bulb temperature.
- RELATIVEHUMIDITY: Loads from the relative humidity.
- INFILTRATIONSENSIBLE: Heat gains and losses from infiltration.
- USERDEFINED: User-defined thermal load type.
- NOTDEFINED: Undefined thermal load type.

> HISTORY: New enumeration in IFC R2.0

EXPRESS specification:

TYPE IfcThermalLoadSourceEnum = ENUMERATION OF
( | PEOPLE, LIGHTING, EQUIPMENT, VENTILATIONINDOORAIR, VENTILATIONOUTSIDEAIR, RECIRCULATEDAIR, EXHAUSTAIR, AIREXCHANGERATE, DRYBULBTEMPERATURE, RELATIVEHUMIDITY, INFILTRATION, USERDEFINED, NOTDEFINED);
END_TYPE;