IfcElectricTimeControlTypeEnum

Definition from IAI: The IfcElectricTimeControlTypeEnum defines the range of types of electrical time control available.

> HISTORY: New type in IFC 2x2

Enumeration

Value | Definition | Pset
TIMECLOCK | A control that causes action to occur at set times. | NO
TIMEDELAY | A control that causes action to occur following a set duration. | NO
RELAY | Electromagnetically operated contactor for making or breaking a control circuit. | NO
USERDEFINED |  |
NOTDEFINED |  |

EXPRESS specification:

TYPE IfcElectricTimeControlTypeEnum = ENUMERATION OF
( | TIMECLOCK, TIMEDELAY, RELAY, USERDEFINED, NOTDEFINED);
END_TYPE;