IfcColourRgb

Definition from ISO/CD 10303-46:1992: A colour rgb as a subtype of colour specifications is defined by three colour component values for red, green, and blue in the RGB colour model.

> NOTE In contrary to the usual value range of colour components being integer from 0...255, the definition from ISO10303-46 defines the colour components as real from 0.0 ... 1.0. Applications need to execute this conversion before populating the colour RGB values.

> NOTE Corresponding STEP name: colour_rgb. The name attribute has been omitted, the data type for the reg, green and blue parts is IfcNormalizedRatioMeasure, that already includes the range restrictions for the values. Please refer to ISO/IS 10303-46:1994, p. 138 for the final definition of the formal standard.

> HISTORY New entity in Release IFC2x Edition 2.

EXPRESS specification:

ENTITY IfcColourRgb
SUBTYPE OF ( | IfcColourSpecification);
Red | : | IfcNormalisedRatioMeasure;
Green | : | IfcNormalisedRatioMeasure;
Blue | : | IfcNormalisedRatioMeasure;
END_ENTITY;

Attribute definitions:

Red | : | The intensity of the red colour component. NOTE&npsp; The colour component value is given within the range of 0..1, and not within the range of 0..255 as otherwise usual.
Green | : | The intensity of the green colour component. NOTE&npsp; The colour component value is given within the range of 0..1, and not within the range of 0..255 as otherwise usual.
Blue | : | The intensity of the blue colour component. NOTE&npsp; The colour component value is given within the range of 0..1, and not within the range of 0..255 as otherwise usual.

Inheritance graph

ENTITY IfcColourRgb;
ENTITY IfcColourSpecification;
Name | : | OPTIONAL IfcLabel;
ENTITY IfcColourRgb;
Red | : | IfcNormalisedRatioMeasure;
Green | : | IfcNormalisedRatioMeasure;
Blue | : | IfcNormalisedRatioMeasure;
END_ENTITY;