IfcMotorConnectionTypeEnum

Definition from IAI: The IfcMotorConnectionTypeEnum defines the range of different types of motor connection that can be specified.

> HISTORY: New type in IFC 2x.

Enumeration

Value | Definition | Pset
BELTDRIVE | An indirect connection made through the medium of a shaped, flexible continuous loop. | NO
COUPLING | An indirect connection made through the medium of the viscosity of a fluid. | NO
DIRECTDRIVE | A direct, physical connection made between the motor and the driven device. | NO
USERDEFINED |  |
NOTDEFINED |  |

EXPRESS specification:

TYPE IfcMotorConnectionTypeEnum = ENUMERATION OF
( | BELTDRIVE, COUPLING, DIRECTDRIVE, USERDEFINED, NOTDEFINED);
END_TYPE;