IfcWasteTerminalTypeEnum

IfcWasteTerminalTypeEnum

Definition from IAI: The IfcWasteTerminalTypeEnum defines the range of different types of waste terminal that can be specified.

> HISTORY: New type in IFC 2x2

Enumeration

Value | Definition | Pset
FLOORTRAP | Pipe fitting, set into the floor, that retains liquid to prevent the passage of foul air | YES
FLOOORWASTE | Pipe fitting, set into the floor, that collects waste water and discharges it to a separate trap. | YES
GULLYSUMP | Pipe fitting or assembly of fittings to receive surface water or waste water, fitted with a grating or sealed cover. | YES
GULLYTRAP | Pipe fitting or assembly of fittings to receive surface water or waste water, fitted with a grating or sealed cover and discharging through a trap (BS6100 330 3504 modified) | YES
GREASEINTERCEPTOR | Chamber, on the line of a drain or discharge pipe, that prevents grease passing into a drainage system (BS6100 330 6205). | YES
OILINTERCEPTOR | One or more chambers arranged to prevent the ingress of oil to a drain or sewer, that retain the oil for later removal (BS6100 330 67316). | YES
PETROLINTERCEPTOR | Two or more chambers with inlet and outlet pipes arranged to allow petrol/gasoline collected on the surface of water drained into them to evaporate through ventilating pipes. | YES
ROOFDRAIN | Pipe fitting, set into the roof, that collects rainwater for discharge into the rainwater system. | YES
WASTEDISPOSALUNIT | Electrically operated device that reduces kitchen or other waste into fragments small enough to be flushed into a drainage system. | YES
WASTETRAP | Pipe fitting, set adjacent to a sanitary terminal, that retains liquid to prevent the passage of foul air. | YES
USERDEFINED |  |
NOTDEFINED |  |

EXPRESS specification:

TYPE IfcWasteTerminalTypeEnum = ENUMERATION OF
( | FLOORTRAP, FLOORWASTE, GULLYSUMP, GULLYTRAP, GREASEINTERCEPTOR, OILINTERCEPTOR, PETROLINTERCEPTOR, ROOFDRAIN, WASTEDISPOSALUNIT, WASTETRAP, USERDEFINED, NOTDEFINED);
END_TYPE;