IFCSTRUCTURALLOADRESOURCE

The data model consists of the following:

| 17 | Entities

The IfcStructuralLoadResource holds the definitions of structural loads, boundary conditions, and connection conditions. These definitions specify the force, moment, stiffness, displacement and other factor, independently of the location, where such loads take effect.

The load resource definitions are used in other parts of the IFC model, including by the definition of structural actions and reactions that places the load definitions into 2D or 3D space.

> NOTE: The current version of IFC does not define dynamic loads, it is restricted to static loads.

> HISTORY: New schema in Release IFC2x Edition 2.

Interfaced schemas (1):

REFERENCE FROM IFCMEASURERESOURCE
( | IfcLabel, IfcLinearStiffnessMeasure, IfcRotationalStiffnessMeasure, IfcForceMeasure, IfcTorqueMeasure, IfcLinearForceMeasure, IfcLinearMomentMeasure, IfcPlanarForceMeasure, IfcLengthMeasure, IfcPlaneAngleMeasure, IfcThermodynamicTemperatureMeasure, IfcModulusOfSubgradeReactionMeasure, IfcWarpingMomentMeasure, IfcModulusOfLinearSubgradeReactionMeasure, IfcModulusOfRotationalSubgradeReactionMeasure, IfcCurvatureMeasure);

Entities (17):

| IfcBoundaryCondition
| IfcBoundaryEdgeCondition
| IfcBoundaryFaceCondition
| IfcBoundaryNodeCondition
| IfcBoundaryNodeConditionWarping
| IfcFailureConnectionCondition
| IfcSlippageConnectionCondition
| IfcStructuralConnectionCondition
| IfcStructuralLoad
| IfcStructuralLoadLinearForce
| IfcStructuralLoadPlanarForce
| IfcStructuralLoadSingleDisplacement
| IfcStructuralLoadSingleDisplacementDistortion
| IfcStructuralLoadSingleForce
| IfcStructuralLoadSingleForceWarping
| IfcStructuralLoadStatic
| IfcStructuralLoadTemperature