IfcModulusOfRotationalSubgradeReactionMeasure

Definition from IAI: A measure for modulus of rotational subgrade reaction, which expresses the rotational elastic bedding of a linear structural element per length, e.g. a beam. It is typically measured in Nm/(m*rad).

Type: REAL

> HISTORY New type in IFC Release 2x2.

EXPRESS specification:

TYPE IfcModulusOfRotationalSubgradeReactionMeasure = REAL;
END_TYPE;