IfcDistributionChamberElementTypeEnum

Definition from IAI: The This enumeration identifies different types of distribution chambers.

Valid enumerations are:

- FORMEDDUCT: Space formed in the ground for the passage of pipes, cables, ducts. (BS6100 100 3410)
- INSPECTIONCHAMBER: Chamber constructed on a drain, sewer or pipeline and with a removable cover, that permits visble inspection..
- INSPECTIONPIT: Recess or chamber formed to permit access for inspection of substructure and services. (BS6100 221 4128 - modified)
- MANHOLE: Chamber constructed on a drain, sewer or pipeline and with a removable cover, that permits the entry of a person.
- METERCHAMBER: Chamber that houses a meter(s) (BS6100 250 6224 - modified)
- SUMP: Recess or small chamber into which liquid is drained to facilitate its removal (BS6100 100 3431)
- TRENCH: Excavation, the length of which greatly exceeds the width. (BS6100 221 4118)
- VALVECHAMBER: Chamber that houses a valve(s) (BS6100 250 6224)
- USERDEFINED: User-defined terminal box.
- NOTDEFINED: Undefined terminal box.

> HISTORY: New enumeration in IFC R2x2

EXPRESS specification:

TYPE IfcDistributionChamberElementTypeEnum = ENUMERATION OF
( | FORMEDDUCT, INSPECTIONCHAMBER, INSPECTIONPIT, MANHOLE, METERCHAMBER, SUMP, TRENCH, VALVECHAMBER, USERDEFINED, NOTDEFINED);
END_TYPE;