IfcFireSuppressionTerminalTypeEnum

Definition from IAI: The IfcFireSuppressionTerminalTypeEnum defines the range of different types of fire suppression terminal that can be specified.

> HISTORY: New type in IFC 2x2

Enumeration

Value | Definition | Pset
BREECHINGINLET | Symmetrical pipe fitting that unites two or more inlets into a single pipe (BS6100 330 114 adapted) | YES
FIREHYDRANT | Device, fitted to a pipe, through which a temporary supply of water may be provided (BS6100 330 6107) | YES
HOSEREEL | A supporting framework on which a hose may be wound (BS6100 155 8201) | YES
SPRINKLER | Device for sprinkling water from a pipe under pressure over an area (BS6100 100 3432) | YES
SPRINKLERDEFLECTOR | Device attached to a sprinkler to deflect the water flow into a spread pattern to cover the required area (IAI) | YES
USERDEFINED |  |
NOTDEFINED |  |

EXPRESS specification:

TYPE IfcFireSuppressionTerminalTypeEnum = ENUMERATION OF
( | BREECHINGINLET, FIREHYDRANT, HOSEREEL, SPRINKLER, SPRINKLERDEFLECTOR, USERDEFINED, NOTDEFINED);
END_TYPE;