#### 5.2.4.8 AISC_EM11_Pset_Castellation

| Castellation: Castellation has a repeating hole feature along its length. The repeating feature may be given by its type. It may also define spacing, height and width.

buildingSMART Data Dictionary

PSD-XML

Name | Type | Description
--- | --- | ---
CastellationType | P_ENUMERATEDVALUE / AISC_EM11_CastellationType |
| Castellation Type | Castellation Type declares the classification of the type of longitudinal repeating feature by its shape. Value can be one of : Circular Hexagonal Octagonal Undefined
CastellationEndPostWidth1 | P_SINGLEVALUE / IfcPositiveLengthMeasure |
| Castellation End Post Width 1 | Castellation End Post Width 1 in IfcLengthMeasure type, provides the numerical value with an appropriate unit of the linear dimension to the first web opening measured from the first cut end.
CastellationEndPostWidth2 | P_SINGLEVALUE / IfcPositiveLengthMeasure |
| Castellation End Post Width 2 | Castellation End Post Width 2 in IfcLengthMeasure type, provides the numerical value with an appropriate unit of the linear dimension to the last web opening measured from the last cut end.
CastellationSpacing | P_SINGLEVALUE / IfcPositiveLengthMeasure |
| Castellation Spacing | Castellation Spacing in IfcLengthMeasure type, specifis the numerical value with an appropriate unit of the linear distance between each feature, measured along the length of the part.
CastellationHeight | P_SINGLEVALUE / IfcPositiveLengthMeasure |
| Castellation Height | Castellation Height in IfcLengthMeasure type, specifies the numerical value with an appropriate unit of the linear distance between the top and bottom of each feature, measured across the depth of the part.
CastellationWidth | P_SINGLEVALUE / IfcPositiveLengthMeasure |
| Castellation Width | Castellation Width in IfcLengthMeasure type, specifies the numerical value with an appropriate unit of the linear distance between the extreme edges of each feature, measured along the length of the part.
CastellationDepth | P_SINGLEVALUE / IfcPositiveLengthMeasure |
| Castellation Depth | Castellation Depth in IfcLengthMeasure type, specifies the numerical value with an appropriate unit of the linear distance between the top of the part and the extreme edges of each feature, measured down the depth of the part.

Link to this page