IfcCableCarrierSegmentTypeEnum

Definition from IAI: The IfcCableCarrierSegmentTypeEnum defines the range of different types of cable carrier segment that can be specified.

> HISTORY: New type in IFC 2x2

Enumeration

Value | Definition | Pset
CABLELADDERSEGMENT | An open carrier segment on which cables are carried on a ladder structure. | YES
CABLETRAYSEGMENT | An (typically) open carrier segment onto which cables are laid. | YES
CABLETRUNKINGSEGMENT | An enclosed carrier segment with one or more compartments into which cables are placed. | YES
CONDUITSEGMENT | An enclosed tubular carrier segment through which cables are pulled. | YES
USERDEFINED |  |
NOTDEFINED |  |

EXPRESS specification:

TYPE IfcCableCarrierSegmentTypeEnum = ENUMERATION OF
( | CABLELADDERSEGMENT, CABLETRAYSEGMENT, CABLETRUNKINGSEGMENT, CONDUITSEGMENT, USERDEFINED, NOTDEFINED);
END_TYPE;