IfcProcedureTypeEnum

Definition from IAI: The IfcProcedureTypeEnum defines the range of different types of procedure that can be specified.

> HISTORY: New type in IFC 2x2

Enumeration

Value | Definition
ADVICE_CAUTION | A caution that should be taken note of as a procedure or when carrying out a procedure.
ADVICE_NOTE | Additional information or advice that should be taken note of as a procedure or when carrying out a procedure.
ADVICE_WARNING | A warning of potential danger that should be taken note of as a procedure or when carrying out a procedure.
CALIBRATION | A procedure undertaken to calibrate an artifact.
SHUTDOWN | A procedure undertaken to shutdown the operation an artifact.
STARTUP | A procedure undertaken to start up the operation an artifact.
USERDEFINED |
NOTDEFINED |

EXPRESS specification:

TYPE IfcProcedureTypeEnum = ENUMERATION OF
( | ADVICE_CAUTION, ADVICE_NOTE, ADVICE_WARNING, CALIBRATION, DIAGNOSTIC, SHUTDOWN, STARTUP, USERDEFINED, NOTDEFINED);
END_TYPE;