#### 5.2.4.7 AISC_EM11_Pset_ToleranceForLayout

| Tolerance for Layout: Geometric tolerencing is implicitly represented through object placement. Object placement specifies relative location and guidance for tolerance measurement. Tolerance value should be represented as property

buildingSMART Data Dictionary

PSD-XML

Name | Type | Description
--- | --- | ---
LayoutTolerance | P_LISTVALUE / IfcLengthMeasure |
| Layout Tolerance | Allowed tolerance value in placement

Link to this page