#### 5.2.4.20 AISC_EM11_Pset_TubeCrossingSaddle

| Tube Crossing Saddle: image source : Tube NC

buildingSMART Data Dictionary

PSD-XML

Name | Type | Description
--- | --- | ---
Type | P_SINGLEVALUE / IfcIdentifier |
MinBurnAngle | P_SINGLEVALUE / IfcPlaneAngleMeasure |
MaxBurnAngle | P_SINGLEVALUE / IfcPlaneAngleMeasure |
Bevel | P_SINGLEVALUE / IfcPlaneAngleMeasure | The bevel is nothing more than a kerf with a continuous opening angle between the cut and connecting material. Internally in the machine software the bevel is created mathematically by calculating the dihedral angle and subtracting the bevel from it.
RootOpening | P_SINGLEVALUE / IfcPositiveLengthMeasure |
Shrinkage | P_SINGLEVALUE / IfcPositiveLengthMeasure |

Link to this page