IfcCableSegmentTypeEnum

Definition from IAI: The IfcCableSegmentTypeEnum defines the range of different types of cable segment that can be specified.

> HISTORY: New type in IFC 2x2

Enumeration

Value | Definition | Pset
CABLESEGMENT | Electrical cable with a specific purpose to lead electric current within a circuit or any other electric construction. Includes all types of electric cables, mainly several electrical segments wrapped together, e.g. cable, tube, busbar. Note that the number of conductors within a cable is determined by an aggregation mechanism that aggregates the conductors within the cable. | YES
CONDUCTORSEGMENT | A single linear element with the specific purpose to lead electric current. The core of one lead is normaly single wired or multiwired which are intertwined. | YES
USERDEFINED |  |
NOTDEFINED |  |

EXPRESS specification:

TYPE IfcCableSegmentTypeEnum = ENUMERATION OF
( | CABLESEGMENT, CONDUCTORSEGMENT, USERDEFINED, NOTDEFINED);
END_TYPE;