IfcElectricalBaseProperties

Definition from IAI: Common definition to capture basic electrical characteristics for use in building services and facilities management.

> HISTORY: New entity in IFC R2.0.

EXPRESS specification:

ENTITY IfcElectricalBaseProperties
SUBTYPE OF ( | IfcEnergyProperties);
ElectricCurrentType | : | OPTIONAL IfcElectricCurrentEnum;
InputVoltage | : | IfcElectricVoltageMeasure;
InputFrequency | : | IfcFrequencyMeasure;
FullLoadCurrent | : | OPTIONAL IfcElectricCurrentMeasure;
MinimumCircuitCurrent | : | OPTIONAL IfcElectricCurrentMeasure;
MaximumPowerInput | : | OPTIONAL IfcPowerMeasure;
RatedPowerInput | : | OPTIONAL IfcPowerMeasure;
InputPhase | : | INTEGER;
END_ENTITY;

Attribute definitions:

ElectricCurrentType | : | Type of electrical current applied
InputVoltage | : | Input electrical potential
InputFrequency | : | Nominal frequency of input voltage wave form.
FullLoadCurrent | : | Full load electrical current requirements.
MinimumCircuitCurrent | : | Minimum current carrying capacity of the electrical circuit.
MaximumPowerInput | : | Maximum power input of the electrical device
RatedPowerInput | : | Actual electrical input power of the electrical device at its rated capacity
InputPhase | : | Relative phase of input conductors

Inheritance graph

ENTITY IfcElectricalBaseProperties;
ENTITY IfcRoot;
GlobalId | : | IfcGloballyUniqueId;
OwnerHistory | : | IfcOwnerHistory;
Name | : | OPTIONAL IfcLabel;
Description | : | OPTIONAL IfcText;
ENTITY IfcPropertyDefinition;
INVERSE
HasAssociations | : | SET OF IfcRelAssociates FOR RelatedObjects;
ENTITY IfcPropertySetDefinition;
INVERSE
PropertyDefinitionOf | : | SET [0:1] OF IfcRelDefinesByProperties FOR RelatingPropertyDefinition;
DefinesType | : | SET [0:1] OF IfcTypeObject FOR HasPropertySets;
ENTITY IfcEnergyProperties;
EnergySequence | : | OPTIONAL IfcEnergySequenceEnum;
UserDefinedEnergySequence | : | OPTIONAL IfcLabel;
ENTITY IfcElectricalBaseProperties;
ElectricCurrentType | : | OPTIONAL IfcElectricCurrentEnum;
InputVoltage | : | IfcElectricVoltageMeasure;
InputFrequency | : | IfcFrequencyMeasure;
FullLoadCurrent | : | OPTIONAL IfcElectricCurrentMeasure;
MinimumCircuitCurrent | : | OPTIONAL IfcElectricCurrentMeasure;
MaximumPowerInput | : | OPTIONAL IfcPowerMeasure;
RatedPowerInput | : | OPTIONAL IfcPowerMeasure;
InputPhase | : | INTEGER;
END_ENTITY;