#### 5.2.4.11 AISC_EM11_Pset_BoltHole

| Bolt Hole: Bolt hole represents a hole mainly used for bolt connection. Propeties can be used for additional information.

buildingSMART Data Dictionary

PSD-XML

Name | Type | Description
--- | --- | ---
FeatureSubType | P_ENUMERATEDVALUE / AISC_EM11_FeatureSubType |
| Feature Sub Type | Feature subtype further specifies the type of hole. Possible values are predefined as in AISC_EM11_FeatureSubType enumerated type. Value can be one of: BeveledHole TappedHole ThreadedHole
BoltHoleDiameter | P_SINGLEVALUE / IfcPositiveLengthMeasure |
| Bolt Hole Diameter | Additional parameterized mapping through IfcPropertySet for diameter.
PartialHoleIndicator | P_SINGLEVALUE / IfcBoolean |
| Partial Hole Indicator | Identification of partial depth hole if the value is set to True.
PartialHoleDepth | P_SINGLEVALUE / IfcPositiveLengthMeasure |
| Partial Hole Depth | The depth of partial depth hole.

Link to this page