IfcElectricFlowStorageDeviceTypeEnum

Definition from IAI: The IfcElectricFlowStorageDeviceTypeEnum defines the range of different types of electrical flow storage device available.

> HISTORY: New type in IFC 2x2

Enumeration

Value | Definition | Pset
BATTERY | A device for storing energy in chemical form so that it can be released as electrical energy. | NO
CAPACITORBANK | A device that stores electrical energy when an external power supply is present using the electrical property of capacitance | NO
HARMONICFILTER | A device that constantly injects currents that precisely correspond to the harmonic components drawn by the load. | NO
UPS | A device that provides a time limited alternative source of power supply in the event of failure of the main supply. | NO
USERDEFINED |  |
NOTDEFINED |  |

EXPRESS specification:

TYPE IfcElectricFlowStorageDeviceTypeEnum = ENUMERATION OF
( | BATTERY, CAPACITORBANK, HARMONICFILTER, INDUCTORBANK, UPS, USERDEFINED, NOTDEFINED);
END_TYPE;